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	Sue Smethurst
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	Our Reference:
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	Construction - Framework
	

	

	

	
	7 Harrington Ave, WARRAWEE NSW 2074
	

	Property:
	
	
	

	
	
	

	

	Inspection Date:
	
	16/11/2017
	

	

	Inspector:
	
	Sheila Inspector Prod
	

	

	

	Report Purpose:
	
	The purpose of this report is to identify defective workmanship or incomplete works as might be expected to be present in a building at Framework stage, in so far as a licensed builder can reasonably identify those defects or faults.

This report is the result of a visual examination only.
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      •    recommend sec 2








richtext00011.rtf
Note: all plumbing services require certification.
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Floor framing - Inspected with Defects / Observations Noted 



Flooring secured - Inspected with Defects / Observations Noted 



Floor sheeting - Inspected with Defects / Observations Noted 



Joist hangers - Inspected with Defects / Observations Noted 



Blocking to floor joists - Inspected with Defects / Observations Noted 



Load bearing stud frames - Inspected & Acceptable
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      •    It was noted there was not a minimum of 2 spans under single sheet flooring.
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      •    rec3
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Framework - Inspected with Defects / Observations Noted 



Connection to the wall - Inspected & Acceptable 



General finish to sheeting - Inspected & Acceptable
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      •    Balcony is incomplete.
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      •    rec 4








richtext00018.rtf
Roof line appears straight - Inspected with Defects / Observations Noted 



Gable framing - Inspected with Defects / Observations Noted 



Roof truss tie down - Inspected & Acceptable 



Bottom cord bracing - Inspected & Acceptable 



Wind bracing to roof trusses - Inspected with Defects / Observations Noted 



Internal wall brackets installed - Inspected & Acceptable 



Battens correct centres and fixing for metal roof - Inspected with Defects / Observations Noted 



Holding down connectors secured correctly - Inspected with Defects / Observations Noted 



Truss boots installed and fixed off - Inspected with Defects / Observations Noted
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      •    comment roof
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      1.  PURPOSE OF INSPECTION

          

          The purpose of the inspection is to provide advice to the Owner of the Property in respect of the Building Works as instructed in the quotation, as per the Terms and Conditions.

          

          

      2.  SCOPE OF INSPECTION

          

          We confirm that the Inspector has reviewed all areas to be inspected as per our Terms and Conditions.

          

          

      3.  DEFECTS

          

          The Inspector has reviewed the Property and prepared this report in accordance with our Terms and Conditions.
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      •    roof comment
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According to The Guide to Standards and Tolerances - undulations in a roof line are considered a defect if the variance is greater than 20mm in a 4m length. The roof line established at the frame stage is not the true test of a defect as the standard applies to the roof line when the roof surface has been completed.
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Column base connection - Not Applicable 



Column top connection - Inspected with Defects / Observations Noted 



Beam to column connections - Inspected with Defects / Observations Noted 



Packing of beams to columns - Inspected with Defects / Observations Noted 



Steel work weather treated as appropriate - Inspected & Acceptable
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      •    steel comment
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      •    steel rec
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The builder's sign was not visible. 



The fences were examined for site security. The condition of the fences was defective. 



The condition of the access gates was defective. 



The temporary erosion control barriers were not effective. 



There was no excess rubbish on site. 



The general condition of the site was organised and tidy.
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      •    comment
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      •    recc
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The site access, kerbs and footpaths were inspected. The kerbs were damaged. 



There was soil on the roadways.
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      •    It is the builder's responsibility to keep paths and roadways clear of site debris.
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There is no additional scope for this inspection report.
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      •    another recommen
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The following are a list of additional items noted during the inspection.
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      •    Items from the previous inspection were checked and noted as satisfactory.

      •    The site is clean and the overall workmanship has been completed to a satisfactory standard. The job is progressing well and the site is ready to proceed to the next stages of construction.
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      •    this is a recommendation
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The inspector was provided with no building plans. 



The inspector was provided with frame and truss plans.
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      •    section 1 comment








richtext00006.rtf


      •    section 1 recommendation
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The installation of wall, floor and roof frames is covered by various standards and manufacturer's reference guides, including Australian Standard AS1684, AS4100, AS/NZS 4600 Cold Formed Steel Structures and AS 4440-2004. Houspect and its inspectors are not certifiers. Assessments in this report are made from a quality assurance perspective with direct reflection to the various standards and where applicable, to The Guide to Standards and Tolerances. 



Note: Items in this report that appear as Not Applicable indicate the item is not relevant or not a part of this building project.
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Wall framing level and plumb - Inspected & Acceptable with a comment 



Wall framing straight - Inspected with Defects / Observations Noted with another comment 



Bulkheads plumb and level - Inspected with Defects / Observations Noted 



Top plate connection - Inspected with Defects / Observations Noted 



Double top plate connection - Inspected with Defects / Observations Noted 



Bottom plate connection - Inspected with Defects / Observations Noted 



Bottom plate overhang slab - Inspected with Defects / Observations Noted 



Suitable bottom plate to floor anchoring - Inspected with Defects / Observations Noted 



Noggins and trimmers - Inspected with Defects / Observations Noted 



Plumbing and service cutouts - Inspected with Defects / Observations Noted 



Critical room dimensions checked (main bathroom / kitchen) - Inspected with Defects / Observations Noted 



Windows and external doors flashed - Inspected with Defects / Observations Noted 



Ceiling heights correct - Inspected with Defects / Observations Noted 



Sheet bracing - Inspected with Defects / Observations Noted Hoop iron bracing installed correctly - Inspected & Acceptable
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      •    Double top plates were not on truss loaded walls.

      •    Trimmers have not been installed in appropriate locations.

      •    Trimmers are not installed at bulkhead / wall positions.

      •    It was noted that the upper floor frames are connected to lower floor frames.

      •    Walls are checked for straightness with a 2m straight edge. Any deviation should not exceed a maximum of 4mm within the length of the straight edge.








